# MODE_CTL in k210_pac::aes - Rust
AES mode register
Keywords: rust, rustlang, rust-lang, MODE_CTL

# Type Definition k210_pac::aes::MODE_CTL

source · [−]

    pub type MODE_CTL = Reg<u32, _MODE_CTL>;

Expand description

AES mode register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see mode_ctl module

## Trait Implementations

source

### impl ResetValue for MODE_CTL

Register mode_ctl `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for MODE_CTL

`read()` method returns mode_ctl::R reader structure

source

### impl Writable for MODE_CTL

`write(|w| ..)` method takes mode_ctl::W writer structure