# k210_pac::i2c0::intr_mask - Rust
Interrupt Mask Register
Keywords: rust, rustlang, rust-lang, intr_mask

# Module k210_pac::i2c0::intr_mask

source · [−]
Expand description

Interrupt Mask Register

## Structs

ACTIVITY_W

Write proxy for field `activity`

GEN_CALL_W

Write proxy for field `gen_call`

RD_REQ_W

Write proxy for field `rd_req`

RX_DONE_W

Write proxy for field `rx_done`

RX_FULL_W

Write proxy for field `rx_full`

RX_OVER_W

Write proxy for field `rx_over`

RX_UNDER_W

Write proxy for field `rx_under`

START_DET_W

Write proxy for field `start_det`

STOP_DET_W

Write proxy for field `stop_det`

TX_ABRT_W

Write proxy for field `tx_abrt`

TX_EMPTY_W

Write proxy for field `tx_empty`

TX_OVER_W

Write proxy for field `tx_over`

## Type Definitions

ACTIVITY_R

Reader of field `activity`

GEN_CALL_R

Reader of field `gen_call`

R

Reader of register intr_mask

RD_REQ_R

Reader of field `rd_req`

RX_DONE_R

Reader of field `rx_done`

RX_FULL_R

Reader of field `rx_full`

RX_OVER_R

Reader of field `rx_over`

RX_UNDER_R

Reader of field `rx_under`

START_DET_R

Reader of field `start_det`

STOP_DET_R

Reader of field `stop_det`

TX_ABRT_R

Reader of field `tx_abrt`

TX_EMPTY_R

Reader of field `tx_empty`

TX_OVER_R

Reader of field `tx_over`

W

Writer for register intr_mask