# RXUICR in k210_pac::spi0 - Rust
Receive FIFO Underflow Interrupt Clear Register
Keywords: rust, rustlang, rust-lang, RXUICR

# Type Definition k210_pac::spi0::RXUICR

source · [−]

    pub type RXUICR = Reg<u32, _RXUICR>;

Expand description

Receive FIFO Underflow Interrupt Clear Register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see rxuicr module

## Trait Implementations

source

### impl ResetValue for RXUICR

Register rxuicr `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for RXUICR

`read()` method returns rxuicr::R reader structure

source

### impl Writable for RXUICR

`write(|w| ..)` method takes rxuicr::W writer structure