# FCR_IIR in k210_pac::uart1 - Rust
FIFO Control Register / Interrupt Identification Register
Keywords: rust, rustlang, rust-lang, FCR_IIR

# Type Definition k210_pac::uart1::FCR_IIR

source · [−]

    pub type FCR_IIR = Reg<u32, _FCR_IIR>;

Expand description

FIFO Control Register / Interrupt Identification Register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see fcr_iir module

## Trait Implementations

source

### impl ResetValue for FCR_IIR

Register fcr_iir `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for FCR_IIR

`read()` method returns fcr_iir::R reader structure

source

### impl Writable for FCR_IIR

`write(|w| ..)` method takes fcr_iir::W writer structure