# SS_SCL_HCNT in k210_pac::i2c0 - Rust
Standard Speed Clock SCL High Count Register
Keywords: rust, rustlang, rust-lang, SS_SCL_HCNT

# Type Definition k210_pac::i2c0::SS_SCL_HCNT

source · [−]

    pub type SS_SCL_HCNT = Reg<u32, _SS_SCL_HCNT>;

Expand description

Standard Speed Clock SCL High Count Register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see ss_scl_hcnt module

## Trait Implementations

source

### impl ResetValue for SS_SCL_HCNT

Register ss_scl_hcnt `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for SS_SCL_HCNT

`read()` method returns ss_scl_hcnt::R reader structure

source

### impl Writable for SS_SCL_HCNT

`write(|w| ..)` method takes ss_scl_hcnt::W writer structure