# SDA_HOLD in k210_pac::i2c0 - Rust
SDA Hold Time Length Register
Keywords: rust, rustlang, rust-lang, SDA_HOLD

# Type Definition k210_pac::i2c0::SDA_HOLD

source · [−]

    pub type SDA_HOLD = Reg<u32, _SDA_HOLD>;

Expand description

SDA Hold Time Length Register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see sda_hold module

## Trait Implementations

source

### impl ResetValue for SDA_HOLD

Register sda_hold `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for SDA_HOLD

`read()` method returns sda_hold::R reader structure

source

### impl Writable for SDA_HOLD

`write(|w| ..)` method takes sda_hold::W writer structure