# FS_SPKLEN in k210_pac::i2c0 - Rust
SS, FS or FM+ spike suppression limit
Keywords: rust, rustlang, rust-lang, FS_SPKLEN

# Type Definition k210_pac::i2c0::FS_SPKLEN

source · [−]

    pub type FS_SPKLEN = Reg<u32, _FS_SPKLEN>;

Expand description

SS, FS or FM+ spike suppression limit

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see fs_spklen module

## Trait Implementations

source

### impl ResetValue for FS_SPKLEN

Register fs_spklen `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for FS_SPKLEN

`read()` method returns fs_spklen::R reader structure

source

### impl Writable for FS_SPKLEN

`write(|w| ..)` method takes fs_spklen::W writer structure