# R in k210_pac::i2c0::comp_param_1 - Rust
Reader of register comp_param_1
Keywords: rust, rustlang, rust-lang, R

# Type Definition k210_pac::i2c0::comp_param_1::R

source · [−]

    pub type R = R<u32, COMP_PARAM_1>;

Expand description

Reader of register comp_param_1

## Implementations

source

### impl R

source

#### pub fn apb_data_width(&self) -> APB_DATA_WIDTH_R

Bits 0:1 - APB_DATA_WIDTH

source

#### pub fn max_speed_mode(&self) -> MAX_SPEED_MODE_R

Bits 2:3 - MAX_SPEED_MODE

source

#### pub fn hc_count_values(&self) -> HC_COUNT_VALUES_R

Bit 4 - HC_COUNT_VALUES

source

#### pub fn intr_io(&self) -> INTR_IO_R

Bit 5 - INTR_IO

source

#### pub fn has_dma(&self) -> HAS_DMA_R

Bit 6 - HAS_DMA

source

#### pub fn encoded_params(&self) -> ENCODED_PARAMS_R

Bit 7 - ENCODED_PARAMS

source

#### pub fn rx_buffer_depth(&self) -> RX_BUFFER_DEPTH_R

Bits 8:15 - RX_BUFFER_DEPTH

source

#### pub fn tx_buffer_depth(&self) -> TX_BUFFER_DEPTH_R

Bits 16:23 - TX_BUFFER_DEPTH