# TAG_IN_FLAG in k210_pac::aes - Rust
Can input tag (when using GCM)
Keywords: rust, rustlang, rust-lang, TAG_IN_FLAG

# Type Definition k210_pac::aes::TAG_IN_FLAG

source · [−]

    pub type TAG_IN_FLAG = Reg<u32, _TAG_IN_FLAG>;

Expand description

Can input tag (when using GCM)

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see tag_in_flag module

## Trait Implementations

source

### impl ResetValue for TAG_IN_FLAG

Register tag_in_flag `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for TAG_IN_FLAG

`read()` method returns tag_in_flag::R reader structure

source

### impl Writable for TAG_IN_FLAG

`write(|w| ..)` method takes tag_in_flag::W writer structure