# RXCTRL in k210_pac::uarths - Rust
Receive Control Register
Keywords: rust, rustlang, rust-lang, RXCTRL

# Type Definition k210_pac::uarths::RXCTRL

source · [−]

    pub type RXCTRL = Reg<u32, _RXCTRL>;

Expand description

Receive Control Register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see rxctrl module

## Trait Implementations

source

### impl ResetValue for RXCTRL

Register rxctrl `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for RXCTRL

`read()` method returns rxctrl::R reader structure

source

### impl Writable for RXCTRL

`write(|w| ..)` method takes rxctrl::W writer structure