# SYNC_LEVEL in k210_pac::gpio - Rust
Sync level registers
Keywords: rust, rustlang, rust-lang, SYNC_LEVEL

# Type Definition k210_pac::gpio::SYNC_LEVEL

source · [−]

    pub type SYNC_LEVEL = Reg<u32, _SYNC_LEVEL>;

Expand description

Sync level registers

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see sync_level module

## Trait Implementations

source

### impl ResetValue for SYNC_LEVEL

Register sync_level `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for SYNC_LEVEL

`read()` method returns sync_level::R reader structure

source

### impl Writable for SYNC_LEVEL

`write(|w| ..)` method takes sync_level::W writer structure