# W in k210_pac::sysctl::peri_reset - Rust
Writer for register peri_reset
Keywords: rust, rustlang, rust-lang, W

# Type Definition k210_pac::sysctl::peri_reset::W

source · [−]

    pub type W = W<u32, PERI_RESET>;

Expand description

Writer for register peri_reset

## Implementations

source

### impl W

source

#### pub fn rom_reset(&mut self) -> ROM_RESET_W<'_>

Bit 0

source

#### pub fn dma_reset(&mut self) -> DMA_RESET_W<'_>

Bit 1

source

#### pub fn ai_reset(&mut self) -> AI_RESET_W<'_>

Bit 2

source

#### pub fn dvp_reset(&mut self) -> DVP_RESET_W<'_>

Bit 3

source

#### pub fn fft_reset(&mut self) -> FFT_RESET_W<'_>

Bit 4

source

#### pub fn gpio_reset(&mut self) -> GPIO_RESET_W<'_>

Bit 5

source

#### pub fn spi0_reset(&mut self) -> SPI0_RESET_W<'_>

Bit 6

source

#### pub fn spi1_reset(&mut self) -> SPI1_RESET_W<'_>

Bit 7

source

#### pub fn spi2_reset(&mut self) -> SPI2_RESET_W<'_>

Bit 8

source

#### pub fn spi3_reset(&mut self) -> SPI3_RESET_W<'_>

Bit 9

source

#### pub fn i2s0_reset(&mut self) -> I2S0_RESET_W<'_>

Bit 10

source

#### pub fn i2s1_reset(&mut self) -> I2S1_RESET_W<'_>

Bit 11

source

#### pub fn i2s2_reset(&mut self) -> I2S2_RESET_W<'_>

Bit 12

source

#### pub fn i2c0_reset(&mut self) -> I2C0_RESET_W<'_>

Bit 13

source

#### pub fn i2c1_reset(&mut self) -> I2C1_RESET_W<'_>

Bit 14

source

#### pub fn i2c2_reset(&mut self) -> I2C2_RESET_W<'_>

Bit 15

source

#### pub fn uart1_reset(&mut self) -> UART1_RESET_W<'_>

Bit 16

source

#### pub fn uart2_reset(&mut self) -> UART2_RESET_W<'_>

Bit 17

source

#### pub fn uart3_reset(&mut self) -> UART3_RESET_W<'_>

Bit 18

source

#### pub fn aes_reset(&mut self) -> AES_RESET_W<'_>

Bit 19

source

#### pub fn fpioa_reset(&mut self) -> FPIOA_RESET_W<'_>

Bit 20

source

#### pub fn timer0_reset(&mut self) -> TIMER0_RESET_W<'_>

Bit 21

source

#### pub fn timer1_reset(&mut self) -> TIMER1_RESET_W<'_>

Bit 22

source

#### pub fn timer2_reset(&mut self) -> TIMER2_RESET_W<'_>

Bit 23

source

#### pub fn wdt0_reset(&mut self) -> WDT0_RESET_W<'_>

Bit 24

source

#### pub fn wdt1_reset(&mut self) -> WDT1_RESET_W<'_>

Bit 25

source

#### pub fn sha_reset(&mut self) -> SHA_RESET_W<'_>

Bit 26

source

#### pub fn rtc_reset(&mut self) -> RTC_RESET_W<'_>

Bit 29