# DMA_SEL1 in k210_pac::sysctl - Rust
DMA handshake selector
Keywords: rust, rustlang, rust-lang, DMA_SEL1

# Type Definition k210_pac::sysctl::DMA_SEL1

source · [−]

    pub type DMA_SEL1 = Reg<u32, _DMA_SEL1>;

Expand description

DMA handshake selector

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see dma_sel1 module

## Trait Implementations

source

### impl ResetValue for DMA_SEL1

Register dma_sel1 `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for DMA_SEL1

`read()` method returns dma_sel1::R reader structure

source

### impl Writable for DMA_SEL1

`write(|w| ..)` method takes dma_sel1::W writer structure