# SWHSDST in k210_pac::dmac::channel - Rust
Channel Software handshake Destination Register
Keywords: rust, rustlang, rust-lang, SWHSDST

# Type Definition k210_pac::dmac::channel::SWHSDST

source · [−]

    pub type SWHSDST = Reg<u64, _SWHSDST>;

Expand description

Channel Software handshake Destination Register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see swhsdst module

## Trait Implementations

source

### impl ResetValue for SWHSDST

Register swhsdst `reset()`’s with value 0

#### type Type = u64

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for SWHSDST

`read()` method returns swhsdst::R reader structure

source

### impl Writable for SWHSDST

`write(|w| ..)` method takes swhsdst::W writer structure