# ALARM_TIME in k210_pac::rtc - Rust
Alarm time information
Keywords: rust, rustlang, rust-lang, ALARM_TIME

# Type Definition k210_pac::rtc::ALARM_TIME

source · [−]

    pub type ALARM_TIME = Reg<u32, _ALARM_TIME>;

Expand description

Alarm time information

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see alarm_time module

## Trait Implementations

source

### impl ResetValue for ALARM_TIME

Register alarm_time `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for ALARM_TIME

`read()` method returns alarm_time::R reader structure

source

### impl Writable for ALARM_TIME

`write(|w| ..)` method takes alarm_time::W writer structure