# R in k210_pac::i2c0::intr_stat - Rust
Reader of register intr_stat
Keywords: rust, rustlang, rust-lang, R

# Type Definition k210_pac::i2c0::intr_stat::R

source · [−]

    pub type R = R<u32, INTR_STAT>;

Expand description

Reader of register intr_stat

## Implementations

source

### impl R

source

#### pub fn rx_under(&self) -> RX_UNDER_R

Bit 0 - RX_UNDER

source

#### pub fn rx_over(&self) -> RX_OVER_R

Bit 1 - RX_OVER

source

#### pub fn rx_full(&self) -> RX_FULL_R

Bit 2 - RX_FULL

source

#### pub fn tx_over(&self) -> TX_OVER_R

Bit 3 - TX_OVER

source

#### pub fn tx_empty(&self) -> TX_EMPTY_R

Bit 4 - TX_EMPTY

source

#### pub fn rd_req(&self) -> RD_REQ_R

Bit 5 - RD_REQ

source

#### pub fn tx_abrt(&self) -> TX_ABRT_R

Bit 6 - TX_ABRT

source

#### pub fn rx_done(&self) -> RX_DONE_R

Bit 7 - RX_DONE

source

#### pub fn activity(&self) -> ACTIVITY_R

Bit 8 - ACTIVITY

source

#### pub fn stop_det(&self) -> STOP_DET_R

Bit 9 - STOP_DET

source

#### pub fn start_det(&self) -> START_DET_R

Bit 10 - START_DET

source

#### pub fn gen_call(&self) -> GEN_CALL_R

Bit 11 - GEN_CALL