# EIGHT_BIT_MODE in k210_pac::kpu - Rust
Eight bit mode
Keywords: rust, rustlang, rust-lang, EIGHT_BIT_MODE

# Type Definition k210_pac::kpu::EIGHT_BIT_MODE

source · [−]

    pub type EIGHT_BIT_MODE = Reg<u64, _EIGHT_BIT_MODE>;

Expand description

Eight bit mode

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see eight_bit_mode module

## Trait Implementations

source

### impl ResetValue for EIGHT_BIT_MODE

Register eight_bit_mode `reset()`’s with value 0

#### type Type = u64

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for EIGHT_BIT_MODE

`read()` method returns eight_bit_mode::R reader structure

source

### impl Writable for EIGHT_BIT_MODE

`write(|w| ..)` method takes eight_bit_mode::W writer structure