# k210_pac::i2c0::con - Rust
Control Register
Keywords: rust, rustlang, rust-lang, con

# Module k210_pac::i2c0::con

source · [−]
Expand description

Control Register

## Structs

ADDR_SLAVE_WIDTH_W

Write proxy for field `addr_slave_width`

MASTER_MODE_W

Write proxy for field `master_mode`

RESTART_EN_W

Write proxy for field `restart_en`

SLAVE_DISABLE_W

Write proxy for field `slave_disable`

SPEED_W

Write proxy for field `speed`

STOP_DET_W

Write proxy for field `stop_det`

TX_EMPTY_W

Write proxy for field `tx_empty`

## Enums

ADDR_SLAVE_WIDTH_A

Slave address width

SPEED_A

Speed

## Type Definitions

ADDR_SLAVE_WIDTH_R

Reader of field `addr_slave_width`

MASTER_MODE_R

Reader of field `master_mode`

R

Reader of register con

RESTART_EN_R

Reader of field `restart_en`

SLAVE_DISABLE_R

Reader of field `slave_disable`

SPEED_R

Reader of field `speed`

STOP_DET_R

Reader of field `stop_det`

TX_EMPTY_R

Reader of field `tx_empty`

W

Writer for register con