# DIR_BIDX in k210_pac::apu - Rust
Direction Sample Buffer Read Index Configure Register (16 directions * 2 values * 4 indices)
Keywords: rust, rustlang, rust-lang, DIR_BIDX

# Type Definition k210_pac::apu::DIR_BIDX

source · [−]

    pub type DIR_BIDX = Reg<u32, _DIR_BIDX>;

Expand description

Direction Sample Buffer Read Index Configure Register (16 directions * 2 values * 4 indices)

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see dir_bidx module

## Trait Implementations

source

### impl ResetValue for DIR_BIDX

Register dir_bidx[%s] `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for DIR_BIDX

`read()` method returns dir_bidx::R reader structure

source

### impl Writable for DIR_BIDX

`write(|w| ..)` method takes dir_bidx::W writer structure