# RX_SAMPLE_DELAY in k210_pac::spi0 - Rust
RX Sample Delay Register
Keywords: rust, rustlang, rust-lang, RX_SAMPLE_DELAY

# Type Definition k210_pac::spi0::RX_SAMPLE_DELAY

source · [−]

    pub type RX_SAMPLE_DELAY = Reg<u32, _RX_SAMPLE_DELAY>;

Expand description

RX Sample Delay Register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see rx_sample_delay module

## Trait Implementations

source

### impl ResetValue for RX_SAMPLE_DELAY

Register rx_sample_delay `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for RX_SAMPLE_DELAY

`read()` method returns rx_sample_delay::R reader structure

source

### impl Writable for RX_SAMPLE_DELAY

`write(|w| ..)` method takes rx_sample_delay::W writer structure