# CONTROL in k210_pac::timer0::channel - Rust
Control Register
Keywords: rust, rustlang, rust-lang, CONTROL

# Type Definition k210_pac::timer0::channel::CONTROL

source · [−]

    pub type CONTROL = Reg<u32, _CONTROL>;

Expand description

Control Register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see control module

## Trait Implementations

source

### impl ResetValue for CONTROL

Register control `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for CONTROL

`read()` method returns control::R reader structure

source

### impl Writable for CONTROL

`write(|w| ..)` method takes control::W writer structure