# CHEN in k210_pac::dmac - Rust
Channel Enable Register
Keywords: rust, rustlang, rust-lang, CHEN

# Type Definition k210_pac::dmac::CHEN

source · [−]

    pub type CHEN = Reg<u64, _CHEN>;

Expand description

Channel Enable Register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see chen module

## Trait Implementations

source

### impl ResetValue for CHEN

Register chen `reset()`’s with value 0

#### type Type = u64

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for CHEN

`read()` method returns chen::R reader structure

source

### impl Writable for CHEN

`write(|w| ..)` method takes chen::W writer structure