# R in k210_pac::i2s0::channel::isr - Rust
Reader of register isr
Keywords: rust, rustlang, rust-lang, R

# Type Definition k210_pac::i2s0::channel::isr::R

source · [−]

    pub type R = R<u32, ISR>;

Expand description

Reader of register isr

## Implementations

source

### impl R

source

#### pub fn rxda(&self) -> RXDA_R

Bit 0 - Status of receiver data avaliable interrupt

source

#### pub fn rxfo(&self) -> RXFO_R

Bit 1 - Status of data overrun interrupt for RX channel

source

#### pub fn txfe(&self) -> TXFE_R

Bit 4 - Status of transmit empty triger interrupt

source

#### pub fn txfo(&self) -> TXFO_R

Bit 5 - Status of data overrun interrupt for the TX channel