# SOBUF_DMA_RDATA in k210_pac::apu - Rust
Read register for DMA to sample-out buffers
Keywords: rust, rustlang, rust-lang, SOBUF_DMA_RDATA

# Type Definition k210_pac::apu::SOBUF_DMA_RDATA

source · [−]

    pub type SOBUF_DMA_RDATA = Reg<u32, _SOBUF_DMA_RDATA>;

Expand description

Read register for DMA to sample-out buffers

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see sobuf_dma_rdata module

## Trait Implementations

source

### impl ResetValue for SOBUF_DMA_RDATA

Register sobuf_dma_rdata `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for SOBUF_DMA_RDATA

`read()` method returns sobuf_dma_rdata::R reader structure

source

### impl Writable for SOBUF_DMA_RDATA

`write(|w| ..)` method takes sobuf_dma_rdata::W writer structure