# MSTICR in k210_pac::spi3 - Rust
Multi-Master Interrupt Clear Register
Keywords: rust, rustlang, rust-lang, MSTICR

# Type Definition k210_pac::spi3::MSTICR

source · [−]

    pub type MSTICR = Reg<u32, _MSTICR>;

Expand description

Multi-Master Interrupt Clear Register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see msticr module

## Trait Implementations

source

### impl ResetValue for MSTICR

Register msticr `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for MSTICR

`read()` method returns msticr::R reader structure

source

### impl Writable for MSTICR

`write(|w| ..)` method takes msticr::W writer structure