# W in k210_pac::i2c0::raw_intr_stat - Rust
Writer for register raw_intr_stat
Keywords: rust, rustlang, rust-lang, W

# Type Definition k210_pac::i2c0::raw_intr_stat::W

source · [−]

    pub type W = W<u32, RAW_INTR_STAT>;

Expand description

Writer for register raw_intr_stat

## Implementations

source

### impl W

source

#### pub fn rx_under(&mut self) -> RX_UNDER_W<'_>

Bit 0 - RX_UNDER

source

#### pub fn rx_over(&mut self) -> RX_OVER_W<'_>

Bit 1 - RX_OVER

source

#### pub fn rx_full(&mut self) -> RX_FULL_W<'_>

Bit 2 - RX_FULL

source

#### pub fn tx_over(&mut self) -> TX_OVER_W<'_>

Bit 3 - TX_OVER

source

#### pub fn tx_empty(&mut self) -> TX_EMPTY_W<'_>

Bit 4 - TX_EMPTY

source

#### pub fn rd_req(&mut self) -> RD_REQ_W<'_>

Bit 5 - RD_REQ

source

#### pub fn tx_abrt(&mut self) -> TX_ABRT_W<'_>

Bit 6 - TX_ABRT

source

#### pub fn rx_done(&mut self) -> RX_DONE_W<'_>

Bit 7 - RX_DONE

source

#### pub fn activity(&mut self) -> ACTIVITY_W<'_>

Bit 8 - ACTIVITY

source

#### pub fn stop_det(&mut self) -> STOP_DET_W<'_>

Bit 9 - STOP_DET

source

#### pub fn start_det(&mut self) -> START_DET_W<'_>

Bit 10 - START_DET

source

#### pub fn gen_call(&mut self) -> GEN_CALL_W<'_>

Bit 11 - GEN_CALL