# TCR in k210_pac::i2s0::channel - Rust
Transmit Configuration Register
Keywords: rust, rustlang, rust-lang, TCR

# Type Definition k210_pac::i2s0::channel::TCR

source · [−]

    pub type TCR = Reg<u32, _TCR>;

Expand description

Transmit Configuration Register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see tcr module

## Trait Implementations

source

### impl ResetValue for TCR

Register tcr `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for TCR

`read()` method returns tcr::R reader structure

source

### impl Writable for TCR

`write(|w| ..)` method takes tcr::W writer structure