# RegisterBlock in k210_pac::apu - Rust
Register block
Keywords: rust, rustlang, rust-lang, RegisterBlock

# Struct k210_pac::apu::RegisterBlock

source · [−]

    #[repr(C)]pub struct RegisterBlock {Show 15 fields
        pub ch_cfg: CH_CFG,
        pub ctl: CTL,
        pub dir_bidx: [DIR_BIDX; 32],
        pub pre_fir0_coef: [PRE_FIR0_COEF; 9],
        pub post_fir0_coef: [POST_FIR0_COEF; 9],
        pub pre_fir1_coef: [PRE_FIR1_COEF; 9],
        pub post_fir1_coef: [POST_FIR1_COEF; 9],
        pub dwsz_cfg: DWSZ_CFG,
        pub fft_cfg: FFT_CFG,
        pub sobuf_dma_rdata: SOBUF_DMA_RDATA,
        pub vobuf_dma_rdata: VOBUF_DMA_RDATA,
        pub int_stat: INT_STAT,
        pub int_mask: INT_MASK,
        pub sat_counter: SAT_COUNTER,
        pub sat_limits: SAT_LIMITS,
    }

Expand description

Register block

## Fields

`ch_cfg: CH_CFG`

0x00 - Channel Config Register

`ctl: CTL`

0x04 - Control Register

`dir_bidx: [DIR_BIDX; 32]`

0x08 - Direction Sample Buffer Read Index Configure Register (16 directions * 2 values * 4 indices)

`pre_fir0_coef: [PRE_FIR0_COEF; 9]`

0x88 - FIR0 pre-filter coefficients

`post_fir0_coef: [POST_FIR0_COEF; 9]`

0xac - FIR0 post-filter coefficients

`pre_fir1_coef: [PRE_FIR1_COEF; 9]`

0xd0 - FIR1 pre-filter coeffecients

`post_fir1_coef: [POST_FIR1_COEF; 9]`

0xf4 - FIR1 post-filter coefficients

`dwsz_cfg: DWSZ_CFG`

0x118 - Downsize Config Register

`fft_cfg: FFT_CFG`

0x11c - FFT Config Register

`sobuf_dma_rdata: SOBUF_DMA_RDATA`

0x120 - Read register for DMA to sample-out buffers

`vobuf_dma_rdata: VOBUF_DMA_RDATA`

0x124 - Read register for DMA to voice-out buffers

`int_stat: INT_STAT`

0x128 - Interrupt Status Register

`int_mask: INT_MASK`

0x12c - Interrupt Mask Register

`sat_counter: SAT_COUNTER`

0x130 - Saturation Counter

`sat_limits: SAT_LIMITS`

0x134 - Saturation Limits

## Auto Trait Implementations

### impl !RefUnwindSafe for RegisterBlock

### impl Send for RegisterBlock

### impl !Sync for RegisterBlock

### impl Unpin for RegisterBlock

### impl UnwindSafe for RegisterBlock

## Blanket Implementations

source

### impl<T> Any for T where
T: 'static + ?Sized,

source

#### fn type_id(&self) -> TypeId

Gets the `TypeId` of `self`. Read more

source

### impl<T> Borrow<T> for T where
T: ?Sized,

const: unstable · source

#### fn borrow(&self) -> &T

Immutably borrows from an owned value. Read more

source

### impl<T> BorrowMut<T> for T where
T: ?Sized,

const: unstable · source

#### fn borrow_mut(&mut self) -> &mut T

Mutably borrows from an owned value. Read more

source

### impl<T> From<T> for T

const: unstable · source

#### fn from(t: T) -> T

Returns the argument unchanged.

source

### impl<T, U> Into<U> for T where
U: From<T>,

const: unstable · source

#### fn into(self) -> U

Calls `U::from(self)`.

That is, this conversion is whatever the implementation of `From<T> for U` chooses to do.

source

### impl<T, U> TryFrom<U> for T where
U: Into<T>,

#### type Error = Infallible

The type returned in the event of a conversion error.

const: unstable · source

#### fn try_from(value: U) -> Result<T, <T as TryFrom<U>>::Error>

Performs the conversion.

source

### impl<T, U> TryInto<U> for T where
U: TryFrom<T>,

#### type Error = <U as TryFrom<T>>::Error

The type returned in the event of a conversion error.

const: unstable · source

#### fn try_into(self) -> Result<U, <U as TryFrom<T>>::Error>

Performs the conversion.