# MWCR in k210_pac::spi3 - Rust
Microwire Control Register
Keywords: rust, rustlang, rust-lang, MWCR

# Type Definition k210_pac::spi3::MWCR

source · [−]

    pub type MWCR = Reg<u32, _MWCR>;

Expand description

Microwire Control Register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see mwcr module

## Trait Implementations

source

### impl ResetValue for MWCR

Register mwcr `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for MWCR

`read()` method returns mwcr::R reader structure

source

### impl Writable for MWCR

`write(|w| ..)` method takes mwcr::W writer structure