# MTIMECMP in k210_pac::clint - Rust
Hart time comparator register
Keywords: rust, rustlang, rust-lang, MTIMECMP

# Type Definition k210_pac::clint::MTIMECMP

source · [−]

    pub type MTIMECMP = Reg<u64, _MTIMECMP>;

Expand description

Hart time comparator register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see mtimecmp module

## Trait Implementations

source

### impl ResetValue for MTIMECMP

Register mtimecmp[%s] `reset()`’s with value 0

#### type Type = u64

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for MTIMECMP

`read()` method returns mtimecmp::R reader structure

source

### impl Writable for MTIMECMP

`write(|w| ..)` method takes mtimecmp::W writer structure